# White-light LED (Light Emitting Diode) ERS-style product (Ellipsoidal)

## General

### The product shall be an Ovation E-260WW as manufactured by Chauvet & Sons, LLC or approved equal.

#### The product shall be high-intensity LED illuminator utilizing Warm White LEDs and DMX control of intensity.

#### The products shall conform to CSA C22.2 No. 166 and UL 1573 stage and studio use as well as UL 8750 LED standards, tested via MET to conform to the aforementioned UL specifications, the product shall hold both MET and CE markings.

#### The product shall comply with the USITT DMX-512 standard.

#### The product shall comply with the current PLASA ANSI E1.20-2010 remote device management (RDM) standard.

#### All LED products shall be provided by a single manufacturer to ensure color consistency.

### Each LED optic shall be spaced for optimal photometric performance.

#### PHYSICAL

### The dimensions of the fixture shall be 19.49 x 11.14 x 18.42 in (495 x 342 x 506 mm) and weigh approximately 20.2 lbs (9.2 kg).

### The following shall be provided:

#### Ovation E-260WWIP fixture

#### Seetronic Powerkon IP65 power cord

#### Required Accessories (sold separately): Lens Tube 5°, 10°, 14°, 19°, 26°, 36°, 50°, 15°-30° Zoom, and 25°-50° Zoom.

### The housing shall have a black finish.

### Power supply, cooling and electronics shall be integral to each product.

### Product housing shall provide a single power/data port for the Chauvet Ovation GR-1IP Gobo Rotator.

### Product housing shall provide an accessory slot for Gobo Size “A” and Gobo Size “B” and Iris.

## Environmental and Agency Compliance

### The product shall conform to UL 1573, CSA C22.2 No. 166, and UL 8750 LED standards, tested via MET to conform to the aforementioned UL specifications, product shall hold MET and CE markings.

### The product shall conform to Part 15 of the FCC rules.

### The product shall be rated for IP65 for outdoor/wet location use.

## Thermal

### Product heat management shall be achieved though forced cooling.

### The product shall utilize advanced thermal management systems to maintain LED life to an average of 70% intensity after 50,000 hours of use.

### The product shall operate in an ambient temperature range of -4° F (-20° C)minimum**,** to 113° F (45° C) maximum, ambient temperature.

## Electrical

### The product shall be equipped with an auto ranging 100 V to 240 V 50/60 Hz internal power supply.

### The product shall support power in and thru operation.

#### Power in shall be via Seetronic Powerkon IP65 input connector.

#### Power thru shall be via Seetronic Powerkon IP65 output connector.

#### Product power wiring and accessory power cables shall be rated to support linking of 7 E-260WW IP products at 120V.

### The product requires power from a non-dim source.

### Products shall have thermal output compensation to prevent thermal shift of color or intensity.

### Product power input shall have current-limiting fuse protection.

### Power supply shall have power factor correction.

### OPTICAL DATA

### The product shall contain a Warm White LED color system to provide color characteristics as described in the Color section below.

### All LEDs used in the product shall be high brightness and proven quality from established and reputable LED manufacturers.

### Manufacturer of LED emitters shall utilize an advanced production LED binning process to maintain color consistency.

### LED emitters should be rated for nominal 50,000-hour LED life to 70% intensity.

### All LED products (100% of each lot) shall undergo a minimum three-hour burn-in test during manufacturing.

### LED system shall comply with all relevant patents.

## Color

### The product shall utilize a minimum of (1) 230 W Warm White LED emitter.

###### The color rendering index (CRI) shall be 97.2 at 3276 K

1. The product shall be able to provide TM 30-18 scores with a Color Fidelity value of Rf 93.6 with a Gamut of Rg 100.1 at 3276K

## Dimming

### The LED system shall use 16-bit nonlinear scaling techniques for high-resolution dimming.

### The product shall have a selectable dimming curve to simulate incandescent dimming curves.

### Dimming curve shall be optimized for smooth dimming over longer timed fades.

### The LED system shall be digitally driven using high-speed pulse width modulation (PWM).

### LED control shall be compatible with broadcast equipment in the following ways:

### PWM control of LED levels shall be imperceptible to video cameras and related equipment.

### PWM shall be capable of being set on the control via on board controls or via RDM from 600 Hz, 1,200 Hz, 2,000 Hz, 4,000 Hz, 6,000 Hz or 25 kHz.

## REQUIRED FEATURE SET

### The product shall offer 4 DMX personalities.

### The product shall offer 4 Fan modes; Auto, On, Off, Silent

### The product shall offer a noise level not to exceed 37.5 dB at 1 meter.

#### The product shall be compatible with industry standard lens tube sizes.

### Products without the required feature set described above shall not be acceptable.

## Control and User interface

### The product shall be USITT DMX 512A-compatible via in and thru 5-Pin IP XLR DMX Connectors.

### The product shall offer control via DMX and RDM.

### The product shall be compatible with the ANSI RDM E1.20 standard.

#### All product functions shall be accessible via RDM protocol for modification from suitably equipped control console or RDM controller.

#### Temperature sensor within the luminaire shall be viewable in real time via RDM and on the control panel of the product.

#### Products not offering RDM compatibility, feature set access or temperature monitoring via RDM shall not be allowed.

### The product shall be equipped with an LED display with 5 lines of text.

### The product shall be equipped with a 4-button user-interface.

### A variable-rate strobe channel shall be provided.

### The product shall offer stand-alone functionality eliminating the need for a console.

#### Product shall ship with 4 Dimmer Modes accessible via user-interface.

#### Product shall ship with 4 auto sequences with speed control accessible as a stand-alone feature.

#### Product shall ship with the ability to control the Chauvet Ovation GR-1IP via user-interface menu and DMX.

#### Product can be linked together with standard DMX cables and controlled from designated master product.

#### Products without stand-alone operation features described above shall not be acceptable.

-END-